HPL edge banding for countertops

The edge bandings is made of high pressure HPL laminate, intended for finishing the edges of the worktops. Colors consistent with the current collection of countertops.

Available formats at the factory

HPL edge banding for countertops

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 4100 |
| 2. | 4100 |
| 3. | 4100 |
| 4. | 4100 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 45 |
| 2. | 35 |
| 3. | 45 |
| 4. | 35 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 0.7 |
| 2. | 0.7 |
| 3. | 0.5 |
| 4. | 0.5 |

|  |  |
| --- | --- |
|  | Structures |
| 1. | MN |
| 2. | MN |
| 3. | CS∙LN∙MA∙MN∙MT∙PU∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙UR∙VT∙WP∙TP |
| 4. | CS∙LN∙MA∙MN∙MT∙PU∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙UR∙VT∙WP∙TP |

Obraz zawierający sklejka, drewniany, Robienie rzeczy z drewna, Deska

Zawartość wygenerowana przez AI może być niepoprawna.