Paper edge banding, single layer

Edging - paper-based veneer with a weight of 140-200g/m2 , impregnated with a mixture of urea-formaldehyde and melamine formaldehyde resins with elastic additives, with or without a finished lacquer coating, in the form of strips rolled up in disks or in the form of a ribbon rolled up in rolls.

Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 200 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 18|19|20|21|22|23|25|26|28|32|40|49 |

Obraz zawierający podłoga, w pomieszczeniu, drewniany, materiał

Zawartość wygenerowana przez AI może być niepoprawna.