Finish foil, double painted

Paper-based veneer with a weight of 50-110g/m2, impregnated with a mixture of urea-formaldehyde and melamine-formaldehyde resins with additives, with or without a lacquer coating, in the form of a web rolled-in coil.

Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 800 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 2100 |

