Reinforced particle board E05

Low emission particleboard core, Type P2 to EN 312, suitable for non load-bearing purposes in dry areas.

Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 2800 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 2100 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 12∙15∙22 |

