High-pressure laminates

Glamour meets everyday practicality! HPL laminates are proof that design and wear resistance, fire protection and easy care do not have to be contradictory! For all who prefer to implement inspirational ideas with no ifs and buts! Durable and aesthetic product for private and public buildings.

Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 4100 |
| 2. | 4105 |
| 3. | 4105 |
| 4. | 4100 |
| 5. | 4100 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 1300 |
| 2. | 1305 |
| 3. | 1305 |
| 4. | 1300 |
| 5. | 1300 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 0.5 |
| 2. | 0.5 |
| 3. | 0.7 |
| 4. | 0.6 |
| 5. | 0.8 |

|  |  |
| --- | --- |
|  | Structures |
| 1. | MT∙PU∙VT |
| 2. | CS∙LN∙MA∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙TP∙UR∙WP |
| 3. | MN |
| 4. | SG |
| 5. | LN∙MA∙MT∙PU∙RW∙SG∙SO∙WP |

Obraz zawierający sklejka, drewno, opalenizna, design

Zawartość wygenerowana przez AI może być niepoprawna.