Kitchen countertop P2 (E profile)

Worktop made of chipboard in accordance with EN 312. Decorative side covered with high-quality HPL, underside protected with antistretch paper. The front edge of the worktop has a 3 mm radius of curvature. The rear edge is protected with a protective edge band. A variant profiled on both sides is also available.  
  
Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 4100 |
| 2. | 4100 |
| 3. | 4100 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 900 |
| 2. | 1200 |
| 3. | 600 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 28∙38 |
| 2. | 28∙38 |
| 3. | 28∙38 |

|  |  |
| --- | --- |
|  | Structures |
| 1. | CS∙LN∙MA∙MN∙MT∙PU∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙UR∙VT∙WP |
| 2. | CS∙LN∙MA∙MN∙MT∙PU∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙UR∙VT∙WP |
| 3. | CS∙LN∙MA∙MN∙MT∙PU∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙UR∙VT∙WP |

Obraz zawierający Drewniany blok, drewniany, sklejka, drewno

Zawartość wygenerowana przez AI może być niepoprawna.