Thin Compact countertop with black core

Compact high pressure laminate with single or double-sided machined longitudinal edge in standard quality according to EN 438-4:CGS for use as a worktop. With uniform black-coloured core, single-sided decorative melamine resin surface and decorative backing.

Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 4100 |
| 2. | 4100 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 1300 |
| 2. | 1300 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 12 |
| 2. | 12 |

|  |  |
| --- | --- |
|  | Structures |
| 1. | UM |
| 2. | SF ∙SL |

Obraz zawierający szary

Zawartość wygenerowana przez AI może być niepoprawna.