Thin UltraFit countertop P5

A thin worktop, the core of which is a P5 wood-based board. The surface of the top is covered with decorative HPL laminate on both sides. Long edges finished with ABS edging 0.8 mm thick using PUR glue.

Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 4100 |
| 2. | 4100 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 600 |
| 2. | 1200 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 13 |
| 2. | 13 |

|  |  |
| --- | --- |
|  | Structures |
| 1. | MA∙CS∙PU∙QR∙SO∙UR |
| 2. | CS∙MA∙PU∙QR∙SO∙UR |

