Light particle board

Reduced density particle board. Light-weight product. Intended for use in door manufacturing. Thanks to their low weight, LightBoard panels are optimally suited for use as door leaf filling. They offer additional acoustic insulation. The processing of LightBoard panels is easy and safe. Their internal structure allows them to be positioned in any direction - longitudinally or transversally.   
  
Available formats at the factory

|  |  |
| --- | --- |
|  | Length (mm) |
| 1. | 2800 |

|  |  |
| --- | --- |
|  | Width (mm) |
| 1. | 2100 |

|  |  |
| --- | --- |
|  | Thickness (mm) |
| 1. | 33 |

Obraz zawierający meble, mata, Beżowy, dywan

Zawartość wygenerowana przez AI może być niepoprawna.