Splash panel P2

Worktop backsplash made of chipboard according to EN 312 It protects the space between the worktop and the top cabinets, protecting it from soiling and at the same time it is a perfect decorative accent. Available in two variants: with decorative laminate on both sides in the storage collection and with decorative laminate on one side in the production variant, where HPL is used on the back side is counteracting  
  
Available formats at the factory

Length (mm): 4100

Width (mm): 600

Thickness (mm): 11

Structures: CS∙LN∙MA∙MN∙MT∙PU∙QR∙QZ∙RW∙SC∙SG∙SK∙SO∙UR∙VT∙WP∙TP

Obraz zawierający brązowe, książka, ziemia, oprawianie książek

Zawartość wygenerowana przez AI może być niepoprawna.